Arduino

Reference Language | Libraries | Comparison | Changes

## Wire Library

This library allows you to communicate with I2C / TWI devices. On the Arduino boards with the R3 layout (1.0 pinout), the SDA (data line) and SCL (clock line) are on the pin headers close to the AREF pin. The Arduino Due has two I2C / TWI interfaces SDA1 and SCL1 are near to the AREF pin and the additional one is on pins 20 and 21. As a reference the table below shows where TWI pins are located on various Arduino boards.
Board | I2C / TWI pins
Uno, Ethernet | A4 (SDA), A5 (SCL)
Mega2560 | 20 (SDA), 21 (SCL)
Leonardo | 2 (SDA), 3 (SCL)
Due | 20 (SDA), 21 (SCL), SDA1, SCL1
As of Arduino 1.0, the library inherits from the Stream functions, making it consistent with other read/write libraries. Because of this, send() and receive() have been replaced with read() and write(). #### Note There are both 7- and 8-bit versions of I2C addresses. 7 bits identify the device, and the eighth bit determines if it's being written to or read from. The Wire library uses 7 bit addresses throughout. If you have a datasheet or sample code that uses 8 bit address, you'll want to drop the low bit (i.e. shift the value one bit to the right), yielding an address between 0 and 127. However the addresses from 0 to 7 are not used because are reserved so the first address that can be used is 8. ### Examples Digital Potentiometer: Control an Analog Devices AD5171 Digital Potentiometer. Master Reader/Slave Writer: Program two Arduino boards to communicate with one another in a Master Reader/Slave Sender configuration via the I2C. Master Writer/Slave receiver:Program two Arduino boards to communicate with one another in a Master Writer/Slave Receiver configuration via the I2C. SFR Ranger Reader: Read an ultra-sonic range finder interfaced via the I2C. ### See also Master Writer Master Reader SFR Ranger Reader Digital Potentiometer | #### Functions begin() requestFrom() beginTransmission() endTransmission() write() available() read() onReceive() onRequest()

Reference Home

Corrections, suggestions, and new documentation should be posted to the Forum.

The text of the Arduino reference is licensed under a Creative Commons Attribution-ShareAlike 3.0 License. Code samples in the reference are released into the public domain.

### Share

### This link has expired.
Please re-subscribe to our Newsletters.

### Subscribe to our Newsletters

Email

Please enter a valid email to subscribe

Arduino Newsletter
Arduino Store Newsletter

### Confirm your email address

We need to confirm your email address.
To complete the subscription, please click the link in the email we just sent you.

Thank you for subscribing!

Arduino
via Egeo 16
Torino, 10131
Italy

###### Newsletter

- ©2015 Arduino
- Copyright Notice
- Contact us
- About us
- Careers