Arduino

Reference Language | Libraries | Comparison | Changes

LiquidCrystal

## createChar()

#### Description

Create a custom character (gylph) for use on the LCD. Up to eight characters of 5x8 pixels are supported (numbered 0 to 7). The appearance of each custom character is specified by an array of eight bytes, one for each row. The five least significant bits of each byte determine the pixels in that row. To display a custom character on the screen, write() its number.

NB : When referencing custom character "0", if it is not in a variable, you need to cast it as a byte, otherwise the compiler throws an error. See the example below.

#### Syntax

lcd.createChar(num, data)

#### Parameters

lcd: a variable of type LiquidCrystal

num: which character to create (0 to 7)

data: the character's pixel data

#### Example

    #include <LiquidCrystal.h>

    LiquidCrystal lcd(12, 11, 5, 4, 3, 2);

    byte smiley[8] = {
      B00000,
      B10001,
      B00000,
      B00000,
      B10001,
      B01110,
      B00000,
    };

    void setup() {
      lcd.createChar(0, smiley);
      lcd.begin(16, 2);
      lcd.write(byte(0));
    }

    void loop() {}

Reference Home

Corrections, suggestions, and new documentation should be posted to the Forum.

The text of the Arduino reference is licensed under a Creative Commons Attribution-ShareAlike 3.0 License. Code samples in the reference are released into the public domain.

### Share

### This link has expired.
Please re-subscribe to our Newsletters.

### Subscribe to our Newsletters

Email

Please enter a valid email to subscribe

Arduino Newsletter
Arduino Store Newsletter

### Confirm your email address

We need to confirm your email address.
To complete the subscription, please click the link in the email we just sent you.

Thank you for subscribing!

Arduino
via Egeo 16
Torino, 10131
Italy

###### Newsletter

- ©2015 Arduino
- Copyright Notice
- Contact us
- About us
- Careers