Arduino

Reference Language | Libraries | Comparison | Changes

## double

#### Description

Double precision floating point number. On the Uno and other ATMEGA based boards, this occupies 4 bytes. That is, the double implementation is exactly the same as the float, with no gain in precision.

On the Arduino Due, doubles have 8-byte (64 bit) precision.

#### Tip

Users who borrow code from other sources that includes double variables may wish to examine the code to see if the implied precision is different from that actually achieved on ATMEGA based Arduinos.

#### See:

- float

Reference Home

Corrections, suggestions, and new documentation should be posted to the Forum.

The text of the Arduino reference is licensed under a Creative Commons Attribution-ShareAlike 3.0 License. Code samples in the reference are released into the public domain.

### Share

### This link has expired.
Please re-subscribe to our Newsletters.

### Subscribe to our Newsletters

Email

Please enter a valid email to subscribe

Arduino Newsletter
Arduino Store Newsletter

### Confirm your email address

We need to confirm your email address.
To complete the subscription, please click the link in the email we just sent you.

Thank you for subscribing!

Arduino
via Egeo 16
Torino, 10131
Italy

###### Newsletter

- ©2015 Arduino
- Copyright Notice
- Contact us
- About us
- Careers