Arduino

Reference Language | Libraries | Comparison | Changes

## LiquidCrystal Library

This library allows an Arduino board to control LiquidCrystal displays (LCDs) based on the Hitachi HD44780 (or a compatible) chipset, which is found on most text-based LCDs. The library works with in either 4- or 8-bit mode (i.e. using 4 or 8 data lines in addition to the rs, enable, and, optionally, the rw control lines). ### Examples Autoscroll: Shift text right and left. Blink: Control of the block-style cursor. Cursor: Control of the underscore-style cursor. Display: Quickly blank the display without losing what's on it. Hello World: Displays "hello world!" and the seconds since reset. Scroll: Scroll text left and right. Serial Display: Accepts serial input, displays it. Set Cursor: Set the cursor position. Text Direction: Control which way text flows from the cursor. | #### Function LiquidCrystal() begin() clear() home() setCursor() write() print() cursor() noCursor() blink() noBlink() display() noDisplay() scrollDisplayLeft() scrollDisplayRight() autoscroll() noAutoscroll() leftToRight() rightToLeft() createChar()

Reference Home

Corrections, suggestions, and new documentation should be posted to the Forum.

The text of the Arduino reference is licensed under a Creative Commons Attribution-ShareAlike 3.0 License. Code samples in the reference are released into the public domain.

### Share

### This link has expired.
Please re-subscribe to our Newsletters.

### Subscribe to our Newsletters

Email

Please enter a valid email to subscribe

Arduino Newsletter
Arduino Store Newsletter

### Confirm your email address

We need to confirm your email address.
To complete the subscription, please click the link in the email we just sent you.

Thank you for subscribing!

Arduino
via Egeo 16
Torino, 10131
Italy

###### Newsletter

- ©2015 Arduino
- Copyright Notice
- Contact us
- About us
- Careers