Arduino

Reference Language | Libraries | Comparison | Changes

## millis()

#### Description

Returns the number of milliseconds since the Arduino board began running the current program. This number will overflow (go back to zero), after approximately 50 days.

#### Parameters

None

#### Returns

Number of milliseconds since the program started (unsigned long)

#### Note:

Please note that the return value for millis() is an unsigned long, logic errors may occur if a programmer tries to do arithmetic with smaller data types such as int's. Even signed long may encounter errors as its maximum value is half that of its unsigned counterpart.

#### Example

unsigned long time;
void setup(){
Serial.begin(9600);
}
void loop(){
Serial.print("Time: ");
time = millis();
//prints time since program started
Serial.println(time);
// wait a second so as not to send massive amounts of data
delay(1000);
}
[Get Code]

#### See also

- micros()
- delay()
- delayMicroseconds()
- Tutorial: Blink Without Delay

Reference Home

Corrections, suggestions, and new documentation should be posted to the Forum.

The text of the Arduino reference is licensed under a Creative Commons Attribution-ShareAlike 3.0 License. Code samples in the reference are released into the public domain.

### Share

### This link has expired.
Please re-subscribe to our Newsletters.

### Subscribe to our Newsletters

Email

Please enter a valid email to subscribe

Arduino Newsletter
Arduino Store Newsletter

### Confirm your email address

We need to confirm your email address.
To complete the subscription, please click the link in the email we just sent you.

Thank you for subscribing!

Arduino
via Egeo 16
Torino, 10131
Italy

###### Newsletter

- ©2015 Arduino
- Copyright Notice
- Contact us
- About us
- Careers