Arduino

Reference Language | Libraries | Comparison | Changes

## min(x, y)

#### Description

Calculates the minimum of two numbers.

#### Parameters

x: the first number, any data type

y: the second number, any data type

#### Returns

The smaller of the two numbers.

#### Examples

sensVal = min(sensVal, 100); // assigns sensVal to the smaller of sensVal or 100
// ensuring that it never gets above 100.
[Get Code]

#### Note

Perhaps counter-intuitively, max() is often used to constrain the lower end of a variable's range, while min() is used to constrain the upper end of the range.

#### Warning

Because of the way the min() function is implemented, avoid using other functions inside the brackets, it may lead to incorrect results

min(a++, 100); // avoid this - yields incorrect results
min(a, 100);
a++; // use this instead - keep other math outside the function
[Get Code]

#### See also

- max()
- constrain()

Reference Home

Corrections, suggestions, and new documentation should be posted to the Forum.

The text of the Arduino reference is licensed under a Creative Commons Attribution-ShareAlike 3.0 License. Code samples in the reference are released into the public domain.

### Share

### This link has expired.
Please re-subscribe to our Newsletters.

### Subscribe to our Newsletters

Email

Please enter a valid email to subscribe

Arduino Newsletter
Arduino Store Newsletter

### Confirm your email address

We need to confirm your email address.
To complete the subscription, please click the link in the email we just sent you.

Thank you for subscribing!

Arduino
via Egeo 16
Torino, 10131
Italy

###### Newsletter

- ©2015 Arduino
- Copyright Notice
- Contact us
- About us
- Careers