Arduino

Reference Language | Libraries | Comparison | Changes

Bridge : Bridge Class

## put()

#### Description

The put() function allows you to store data on the Linux processor using a Key/Value structure. The Key field is like a label and you can associate a value to it. The key name must be unique in order to identify the correct value. On the Linux side there is a data store where all the keys and the values are saved.

The datastore is saved in the RAM of the AR9331, you will lose the datastore when you restart the bridge software on the Linux side (through power cycling, resetting the Linux processor, or uploading a sketch through WiFi or Ethernet). You will not lose the datastore if you reset the ATMega32u4 processor.

#### Syntax

bridge.put(key, value)

#### Parameters

key: char or string, the key name you want to assign to identify the value.

value: char or string, the value you want to store.

#### Returns

None

#### See Also

- Bridge.get()

Reference Home

Corrections, suggestions, and new documentation should be posted to the Forum.

The text of the Arduino reference is licensed under a Creative Commons Attribution-ShareAlike 3.0 License. Code samples in the reference are released into the public domain.

### Share

### This link has expired.
Please re-subscribe to our Newsletters.

### Subscribe to our Newsletters

Email

Please enter a valid email to subscribe

Arduino Newsletter
Arduino Store Newsletter

### Confirm your email address

We need to confirm your email address.
To complete the subscription, please click the link in the email we just sent you.

Thank you for subscribing!

Arduino
via Egeo 16
Torino, 10131
Italy

###### Newsletter

- ©2015 Arduino
- Copyright Notice
- Contact us
- About us
- Careers