Arduino

Reference Language | Libraries | Comparison | Changes

## WiFi library

The firmware for the WiFi shield has changed in Arduino IDE 1.0.5. You are recommended to install this update per these instructions With the Arduino WiFi Shield, this library allows an Arduino board to connect to the internet. It can serve as either a server accepting incoming connections or a client making outgoing ones. The library supports WEP and WPA2 Personal encryption, but not WPA2 Enterprise. Also note, if the SSID is not broadcast, the shield cannot connect. Arduino communicates with the WiFi shield using the SPI bus. This is on digital pins 11, 12, and 13 on the Uno and pins 50, 51, and 52 on the Mega. On both boards, pin 10 is used as SS. On the Mega, the hardware SS pin, 53, is not used but it must be kept as an output or the SPI interface won't work. Digital pin 7 is used as a handshake pin between the Wifi shield and the Arduino, and should not be used. The WiFi library is very similar to the Ethernet library, and many of the function calls are the same. For additional information on the WiFi shield, see the Getting Started page and the WiFi shield hardware page. ### Examples ConnectNoEncryption : Demonstrates how to connect to an open network ConnectWithWEP : Demonstrates how to connect to a network that is encrypted with WEP ConnectWithWPA : Demonstrates how to connect to a network that is encrypted with WPA2 Personal ScanNetworks : Displays all WiFi networks in range WiFiChatServer : Set up a simple chat server WiFiWebClient : Connect to a remote webserver WiFiWebClientRepeating : Make repeated HTTP calls to a webserver WiFiWebServer : Serve a webpage from the WiFi shield WiFiSendReceiveUDPString : Send and receive a UDP string UdpNTPClient : Query a Network Time Protocol (NTP) server using UDP | #### WiFi class The WiFi class initializes the ethernet library and network settings. begin() disconnect() config() setDNS() SSID() BSSID() RSSI() encryptionType() scanNetworks() status() getSocket() macAddress() #### IPAddress class The IPAddress class provides information about the network configuration. localIP() subnetMask() gatewayIP() #### Server class The Server class creates servers which can send data to and receive data from connected clients (programs running on other computers or devices). Server WiFiServer() begin() available() write() print() println() #### Client class The client class creates clients that can connect to servers and send and receive data. Client WiFiClient() connected() connect() write() print() println() available() read() flush() stop() #### UDP class The UDP class enables UDP message to be sent and received. WiFiUDP begin() available() beginPacket() endPacket() write() parsePacket() peek() read() flush() stop() remoteIP() remotePort()

Reference Home

Corrections, suggestions, and new documentation should be posted to the Forum.

The text of the Arduino reference is licensed under a Creative Commons Attribution-ShareAlike 3.0 License. Code samples in the reference are released into the public domain.

### Share

### This link has expired.
Please re-subscribe to our Newsletters.

### Subscribe to our Newsletters

Email

Please enter a valid email to subscribe

Arduino Newsletter
Arduino Store Newsletter

### Confirm your email address

We need to confirm your email address.
To complete the subscription, please click the link in the email we just sent you.

Thank you for subscribing!

Arduino
via Egeo 16
Torino, 10131
Italy

###### Newsletter

- ©2015 Arduino
- Copyright Notice
- Contact us
- About us
- Careers