Arduino

Reference Language | Libraries | Comparison | Changes

SD : File class

## rewindDirectory()

rewindDirectory() will bring you back to the first file in the directory, used in conjunction with openNextFile().

#### Syntax

file.rewindDirectory()

#### Parameters

file: an instance of the File class.

#### Returns

None

#include <SD.h>
File root;
void setup()
{
Serial.begin(9600);
pinMode(10, OUTPUT);
SD.begin(10);
root = SD.open("/");
printDirectory(root, 0);
Serial.println("done!");
}
void loop()
{
// nothing happens after setup finishes.
}
void printDirectory(File dir, int numTabs) {
while(true) {
File entry = dir.openNextFile();
if (! entry) {
// no more files
// return to the first file in the directory
dir.rewindDirectory();
break;
}
for (uint8_t i=0; i<numTabs; i++) {
Serial.print('\t');
}
Serial.print(entry.name());
if (entry.isDirectory()) {
Serial.println("/");
printDirectory(entry, numTabs+1);
} else {
// files have sizes, directories do not
Serial.print("\t\t");
Serial.println(entry.size(), DEC);
}
}
}
[Get Code]

#### See Also

- open()
- openNextFile()
- isDirectory()

Reference Home

Corrections, suggestions, and new documentation should be posted to the Forum.

The text of the Arduino reference is licensed under a Creative Commons Attribution-ShareAlike 3.0 License. Code samples in the reference are released into the public domain.

### Share

### This link has expired.
Please re-subscribe to our Newsletters.

### Subscribe to our Newsletters

Email

Please enter a valid email to subscribe

Arduino Newsletter
Arduino Store Newsletter

### Confirm your email address

We need to confirm your email address.
To complete the subscription, please click the link in the email we just sent you.

Thank you for subscribing!

Arduino
via Egeo 16
Torino, 10131
Italy

###### Newsletter

- ©2015 Arduino
- Copyright Notice
- Contact us
- About us
- Careers