Arduino

Reference Language | Libraries | Comparison | Changes

## micros()

#### Description

Returns the number of microseconds since the Arduino board began running the current program. This number will overflow (go back to zero), after approximately 70 minutes. On 16 MHz Arduino boards (e.g. Duemilanove and Nano), this function has a resolution of four microseconds (i.e. the value returned is always a multiple of four). On 8 MHz Arduino boards (e.g. the LilyPad), this function has a resolution of eight microseconds.

Note: there are 1,000 microseconds in a millisecond and 1,000,000 microseconds in a second.

#### Parameters

None

#### Returns

Number of microseconds since the program started (unsigned long)

#### Example

    unsigned long time;

    void setup(){
      Serial.begin(9600);
    }
    void loop(){
      Serial.print("Time: ");
      time = micros();
      //prints time since program started
      Serial.println(time);
      // wait a second so as not to send massive amounts of data
      delay(1000);
    }

#### See also

- millis()
- delay()
- delayMicroseconds()

Reference Home

Corrections, suggestions, and new documentation should be posted to the Forum.

The text of the Arduino reference is licensed under a Creative Commons Attribution-ShareAlike 3.0 License. Code samples in the reference are released into the public domain.

### Share

### This link has expired.
Please re-subscribe to our Newsletters.

### Subscribe to our Newsletters

Email

Please enter a valid email to subscribe

Arduino Newsletter
Arduino Store Newsletter

### Confirm your email address

We need to confirm your email address.
To complete the subscription, please click the link in the email we just sent you.

Thank you for subscribing!

Arduino
via Egeo 16
Torino, 10131
Italy

###### Newsletter

- ©2015 Arduino
- Copyright Notice
- Contact us
- About us
- Careers