Arduino

Reference Language | Libraries | Comparison | Changes

GSM : GSM_SMS class

## write()

#### Description

Writes a character to a SMS message.

#### Syntax

SMS.write(val)

#### Parameters

val: a character to send in the message

#### Returns

byte - write() will return the number of bytes written, though reading that number is optional

#### Example

#include <GSM.h>
#define PINNUMBER ""
// initialize the library instance
GSM gsmAccess; // include a 'true' parameter for debug enabled
GSM_SMS sms;
void setup()
{
// initialize serial communications
Serial.begin(9600);
Serial.println("SMS Messages Sender");
// connection state
boolean notConnected = true;
// Start GSM shield
// If your SIM has PIN, pass it as a parameter of begin() in quotes
while(notConnected)
{
if(gsmAccess.begin(PINNUMBER)==GSM_READY)
notConnected = false;
else
{
Serial.println("Not connected");
delay(1000);
}
}
Serial.println("GSM initialized");
}
void loop()
{
Serial.print("Enter a mobile number: ");
char remoteNumber[20]; // telephone number to send sms
readSerial(remoteNumber);
Serial.println(remoteNumber);
// sms text
Serial.print("Now, enter SMS content: ");
char txtMsg[200];
readSerial(txtMsg);
Serial.println("SENDING");
Serial.println();
Serial.println("Message:");
Serial.println(txtMsg);
// send the message
sms.beginSMS(remoteNumber);
sms.print(txtMsg);
sms.endSMS();
Serial.println("\nCOMPLETE!\n");
}
/*
Read input serial
*/
int readSerial(char result[])
{
int i = 0;
while(1)
{
while (Serial.available() > 0)
{
char inChar = Serial.read();
if (inChar == '\n')
{
result[i] = '\0';
Serial.flush();
return 0;
}
if(inChar!='\r')
{
result[i] = inChar;
i++;
}
}
}
}
[Get Code]

#### See Also

- beginSMS()
- ready()
- endSMS()
- available()
- remoteNumber()
- read()
- write()
- print()
- peek()
- flush()

Reference Home

Corrections, suggestions, and new documentation should be posted to the Forum.

The text of the Arduino reference is licensed under a Creative Commons Attribution-ShareAlike 3.0 License. Code samples in the reference are released into the public domain.

### Share

### This link has expired.
Please re-subscribe to our Newsletters.

### Subscribe to our Newsletters

Email

Please enter a valid email to subscribe

Arduino Newsletter
Arduino Store Newsletter

### Confirm your email address

We need to confirm your email address.
To complete the subscription, please click the link in the email we just sent you.

Thank you for subscribing!

Arduino
via Egeo 16
Torino, 10131
Italy

###### Newsletter

- ©2015 Arduino
- Copyright Notice
- Contact us
- About us
- Careers