Arduino

Reference Language | Libraries | Comparison | Changes

## readBytes()

#### Description

readBytes() read characters from a stream into a buffer. The function terminates if the determined length has been read, or it times out (see setTimeout()).

readBytes() returns the number of bytes placed in the buffer. A 0 means no valid data was found.

This function is part of the Stream class, and is called by any class that inherits from it (Wire, Serial, etc). See the Stream class main page for more information.

#### Syntax

stream.readBytes(buffer, length)

#### Parameters

stream : an instance of a class that inherits from Stream.
buffer: the buffer to store the bytes in (char[] or byte[])
length : the number of bytes to read (int)

#### Returns

The number of bytes placed in the buffer

#### See also

- Stream

Reference Home

Corrections, suggestions, and new documentation should be posted to the Forum.

The text of the Arduino reference is licensed under a Creative Commons Attribution-ShareAlike 3.0 License. Code samples in the reference are released into the public domain.

### Share

### This link has expired.
Please re-subscribe to our Newsletters.

### Subscribe to our Newsletters

Email

Please enter a valid email to subscribe

Arduino Newsletter
Arduino Store Newsletter

### Confirm your email address

We need to confirm your email address.
To complete the subscription, please click the link in the email we just sent you.

Thank you for subscribing!

Arduino
via Egeo 16
Torino, 10131
Italy

###### Newsletter

- ©2015 Arduino
- Copyright Notice
- Contact us
- About us
- Careers